120/01 N13/PANEL CUBICLES – UNFRAMED

Drawing reference(s):

* Manufacturer and reference: Rearo Laminates, 29 Loanbank Quadrant, Glasgow, G51 3HZ.

Tel 0141 440 0800. E-mail [commercial@rearo.co.uk](mailto:commercial@rearo.co.uk). URL [www.rearocommercial.co.uk](http://www.rearocommercial.co.uk).

* Product: ‘**RapidFit MR MFC’**
* Board/panel type: 600kg/m³ grade MR MFC (moisture resistant Melamine Faced Chipboard).
* Panel thickness: 19mm nominal.
* Edge treatment: 2mm matching ABS.
* Range height: 1950mm FFL.
* Panel height: 1800mm.
* Depth: 1525mm (1500mm deep partition panels).
* Floor clearance: 150mm.
* Pedestal adjustment: ± 20mm.
* Pedestal: Aluminium, painted Nickel finish.
* Headrail: Aluminium slimline ‘U’ channel with no visible fixings. Painted Nickel finish.
* Hinges: Aluminium lift off, gravity hinges with front caps. Painted Nickel finish.
* Indicator bolt and keeper: Aluminium slide action lock with no visible fixings. Circular flush fitting faceplate and emergency release facility. Painted Nickel finish.
* Wall fixings: Aluminium ‘U’ brackets painted Nickel finish with bolt through fixings.
* Colour choice: 9 colours from the RapidFit range.
* Accessories: Full length hinge available to conceal any door cuts made on site. Full length ‘U’ channels available to conceal any pilasters/partition cuts made on site.

*Stocked size options*

* Doors (670mm)
* Pilasters (400mm, 250mm, 190mm, 125mm, 85mm)
* Partitions (1500mm)

*Notes*

*All cubicle panels are supplied ‘off the shelf’ and required to be altered on site.*